|  |  |  |
| --- | --- | --- |
| **Configure Vault Printer** | cid:image001.jpg@01D31833.FDEEF110 | Select ADD A LOCAL PRINTER |
|  | cid:image002.jpg@01D31833.FDEEF110 | Select the desired port under USE AN EXISTING PORT |
|  | cid:image003.jpg@01D31833.FDEEF110 | Scroll down to GENERIC and select GENERIC / TEXT ONLY and select NEXT |
|  | cid:image004.jpg@01D31833.FDEEF110 | Give the printer a name. E.G EFTPOS and select NEXT |
|  | cid:image005.jpg@01D31833.FDEEF110 | Select DO NOT SHARE THIS PRINTER  and then NEXT unless you are looking to print the eftpos receipts from multiple lanes on this printer |
|  | cid:image006.jpg@01D31833.FDEEF110 | Untick SET AS THE DEFAULT PRINTER and select FINISH |
|  | cid:image007.png@01D31833.FDEEF110 | Right click the new printer and select PRINTER PROPERTIES |
|  | cid:image008.jpg@01D31833.FDEEF110 | Select the DEVICE SETTINGS tab and change CUT SHEET to NOT AVAILABLE and select APPLY |
|  | cid:image009.jpg@01D31833.FDEEF110 | Select the ADVANCED tab and select PRINTING DEFAULTS |
|  | cid:image010.jpg@01D31833.FDEEF110 | Select the PAPER/QUALITY tab and select CUT SHEET and then APPLY. Click OK to close |
|  | cid:image011.jpg@01D31833.FDEEF110 | Select the PRINTER COMMANDS tab and enter in the below commands:  BEGIN PRINT JOB:  <0D1B0D1B0D1B>  END PRINT JOB:  <0A0D1B0D1B0D1B>d<041D>V<00>  Click APPLY and then OK |
|  | cid:image012.jpg@01D31833.FDEEF110cid:image013.jpg@01D31833.FDEEF110 | Reconfigure the Vault lane and select WINDOWS PRINTER and the EFTPOS printer you just created. If requested for MARGIN settings set these to 0mm |